## 924 ADMIXTURES FOR CONCRETE.

(REV 3-1-17) (FA 3-3-17) (7-17)

SUBARTICLE 924-2.1 is deleted and the following substituted:

**924-2.1 Approved Product List (APL):** The Department maintains a list of qualified admixtures for air-entraining, water-reducing (Type A), accelerating (Type C), water-reducing and retarding (Type D), water-reducer and accelerating (Type E), high range water reducing (Type F) and high range water-reducing and retarding (Type G), high range water-reducing (Type I - Plasticizing and Type II - Plasticizing and retarding) in producing flowing concrete, specific performance (Type S), and corrosion inhibitor, which have been determined as meeting requirements for use on Department projects. Admixtures included on this list, will be permitted without further testing.

The inclusion of any specific product on the APL, as specified in 6-1, indicates that the product has been given contingent approval, as evidenced by previous tests and apparent effectiveness under field conditions.

Except as specified in Sections 346 and 347, no further testing will be required for any product on the APL unless there is indication in actual field use of inadequate or unreliable results.